[VERSIO]
VersMetaDades=5
SubVersMetaDades=0
Vers=4
SubVers=3

[METADADES]
language=eng
MDIdiom=eng
dateStamp=20160606 12063303-0800
characterSet=006
nOrganismes=1
FileIdentifier=LST_20110512_24949

[METADADES:ORGANISME_1]
role=009
OrganisationName=Geophysical Institute. University of Alaska Fairbanks
IndividualName=Jordi Cristóbal

[IDENTIFICATION]
topicCategory=004,007,012
n_keywords=3
AlternateTitle1=LST
language=eng
code=http://www.hyperspectral.alaska.edu/resources_data_products.html
codeSpace=
DatasetTitle=Landsat-5 TM Land surface temperature retrieval
keyword_type1=1
keyword1=land surface temperature
keyword_type2=1
keyword2=surface energy balance
keyword_type3=1
keyword3=hydrology

[OVERVIEW:ASPECTES_TECNICS]
columns=12781
rows=10741

[SPATIAL_REFERENCE_SYSTEM:HORIZONTAL]
HorizontalSystemIdentifier=UTM-6N-WGS84
resolution=30
EquivalentScaleDenominator=50000

[EXTENT]
MinX=295485
MaxX=678915
MinY=7107585
MaxY=7429815
toler_env=0

[OVERVIEW]
CreationDate=20160622 12054650-0800
nConstraints=0
summary=Land surface temperature retrieval from 12 May 2011 using Landsat-5 TM imagery and water vapour from the MODIS product MOD05 though a single channel methodology.
purpose=Land surface temperature estimation

[ATTRIBUTE_DATA]
TipusCompressio=uinteger
unitats=K *0.01
NODATA=-65535
NODATADef=Background value
IluminationElevationAngle=47.1096944468227
IluminationAzimuthAngle=163.464327164043
TipusRelacio=RELACIO_1_N_DICC
unitatsWavelength=µm
BitsPerValue=8
ToneGradation=255
CalibRadiom=3
unitatsL=W/(m²*sr*µm)
IndexsNomsCamps=3-R
NomCamp_3-R=1

[OVERVIEW:ASPECTES_TECNICS:PLAT_INSTR_INFO]
MissionName=5
PlatformFullName=Landsat
PlatformShortName=Landsat
InstrumentFullName=Thematic Mapper
InstrumentShortName=TM

[QUALITY:LINEAGE:PROCESS1]
nOrganismes=1
history=tifimg.exe
purpose=GLOVIS Landsat Data import (from TIFF to MiraMon file format)
date=20140528 12054371-0800

[QUALITY:LINEAGE:PROCESS1:ORGANISME_1]
IndividualName=Jordi Cristóbal
PositionName=Research Assistant Professor
OrganisationName=Geophysical Institute. University of Alaska Fairbanks
phoneVoice1=(+1)907-474-1522
deliveryPoint1=Geophysical Institute. University of Alaska Fairbanks. 903 Koyukuk Dr; Fairbanks, AK 99775-7320; USA.

[QUALITY:LINEAGE:PROCESS2]
nOrganismes=1
history=corrad.exe
purpose=Radiometric correction of Remote Sensing images using "Pons, X.; Pesquer, L.; Cristóbal, J.; González-Guerrero, O. Automatic and improved radiometric correction of landsat imagery using reference values from modis surface reflectance images. Int J Appl Earth Obs 2014, 33, 243-254" methodology.
date=20141202 14170552-0900

[QUALITY:LINEAGE:PROCESS2:ORGANISME_1]
IndividualName=Jordi Cristóbal
PositionName=Research Assistant Professor
OrganisationName=Geophysical Institute. University of Alaska Fairbanks
phoneVoice1=(+1)907-474-1522
deliveryPoint1=Geophysical Institute. University of Alaska Fairbanks. 903 Koyukuk Dr; Fairbanks, AK 99775-7320; USA.

[QUALITY:LINEAGE:PROCESS3]
nOrganismes=1
history=calcimg.exe
purpose=NDVI computation using Landsat bands 4 and 3 following: (band4-band3)/(band4+band3)
date=20141202 14170552-0900

[QUALITY:LINEAGE:PROCESS3:ORGANISME_1]
IndividualName=Jordi Cristóbal
PositionName=Research Assistant Professor
OrganisationName=Geophysical Institute. University of Alaska Fairbanks
phoneVoice1=(+1)907-474-1522
deliveryPoint1=Geophysical Institute. University of Alaska Fairbanks. 903 Koyukuk Dr; Fairbanks, AK 99775-7320; USA.

[QUALITY:LINEAGE:PROCESS4]
nOrganismes=1
history=emissiv.exe
purpose=Land surface emissivity computation according to "Sobrino, J.A.; Jimenez-Munoz, J.C.; Soria, G.; Romaguera, M.; Guanter, L.; Moreno, J.; Plaza, A.; Martincz, P. Land surface emissivity retrieval from different vnir and tir sensors. Ieee T Geosci Remote 2008, 46, 316-327"
date=20141202 14170552-0900

[QUALITY:LINEAGE:PROCESS4:ORGANISME_1]
IndividualName=Jordi Cristóbal
PositionName=Research Assistant Professor
OrganisationName=Geophysical Institute. University of Alaska Fairbanks
phoneVoice1=(+1)907-474-1522
deliveryPoint1=Geophysical Institute. University of Alaska Fairbanks. 903 Koyukuk Dr; Fairbanks, AK 99775-7320; USA.

[QUALITY:LINEAGE:PROCESS5]
nOrganismes=1
history=TST.exe
purpose=Land surface temperature retrieval according to "Jimenez; Cristóbal, J. Revision of the single-channel algorithm fo  land surface temperature retrieval from landsat thermal-infrared data. Ieee T Geosci Remote 2009" and "Cristóbal, J.; Jiménez-Muñoz, J.C.; Sobrino, J.A.; Ninyerola, M.; Pons, X. Improvements in land surface temperature retrieval from the landsat series thermal band using water vapor and air temperature. Journal of Geophysical Research 2009, 114"
date=20141202 14170552-0900

[QUALITY:LINEAGE:PROCESS5:ORGANISME_1]
IndividualName=Jordi Cristóbal
PositionName=Research Assistant Professor
OrganisationName=Geophysical Institute. University of Alaska Fairbanks
phoneVoice1=(+1)907-474-1522
deliveryPoint1=Geophysical Institute. University of Alaska Fairbanks. 903 Koyukuk Dr; Fairbanks, AK 99775-7320; USA.

[DISTRIBUTION_INFO:ORGANISME_1]
IndividualName=Jordi Cristóbal
PositionName=Research Assistant Professor
OrganisationName=Geophysical Institute. University of Alaska Fairbanks
phoneVoice1=(+1)907-474-1522
city=Fairbanks
administrativeArea=Alaska
postalCode=99775
country=USA
electronicMailAddress1=j.cristobal@alaska.edu
n_onlineResource=1
nFormat=1
nTransferOptions=1
nOrderProcess=1

[DISTRIBUTION_INFO:ORGANISME_1:ONLINE_RESOURCE_1]
linkage=http://www.hyperspectral.alaska.edu/resources_data_products.html
function=001

[DISTRIBUTION_INFO:ORGANISME_1:FORMAT_1]
name=MiraMon
fileDecompressionTechnique=None

[DISTRIBUTION_INFO:ORGANISME_1:TRANSFER_OPTIONS_1]
unitsOfDistribution=Alaska
n_onlineResource=1

[DISTRIBUTION_INFO:ORGANISME_1:TRANSFER_OPTIONS_1:ONLINE_RESOURCE_1]
linkage=http://www.hyperspectral.alaska.edu/resources_data_products.html
function=001

[DISTRIBUTION_INFO:ORGANISME_1:ORDER_PROCESS_1]
fees=Free distribution

[DISTRIBUTION_INFO]
nDistributors=1

[ATTRIBUTE_DATA:1]
descriptor=LST
min=19580
max=30473

[ATTRIBUTE_DATA:1:BAND]
MinimumWavelength=10.4
MaximumWavelength=12.5
DN2L_ScaleFactorCoefficient=0.0553740157480315
DN2L_OffsetCoefficient=1.18262598425197
MinL=1.238
MaxL=15.303
